**PLUME COUNTY AIR POLLUTION CONTROL REGULATIONS**

**(Excerpts from EPA CFR 61.145 - STANDARD FOR DEMOLITION/RENOVATION OF BUILDINGS WITH ASBESTOS-CONTAINING MATERIALS)**

**40 CFR 61.145(a)(c**) - A survey to identify the presence and location of asbestos containing materials must be completed prior to demolition or renovation at any business location. The owner of the business shall keep a copy of the report of this survey on file for two years after the demolition is completed.

**40 CFR 61.145(a)(1)** - If the demolition or renovation project will remove more than 260 linear feet of asbestos piping material or 15 square feet of asbestos containing material then the owner and/or certified contractor must comply with the remaining sections of 40 CFR 61.145- DEMOLITION/RENOVATION OF BUILDINGS WITH ASBESTOS-CONTAINING MATERIALS.

**40 CFR 61.145(b)(4)(xiii)**- Removal of asbestos containing material must be performed by a certified contractor or employees of the affected business if they are certified. Certification can be obtained by attending 40 hours of asbestos removal training from an accredited training program and passing the Plume County Air Pollution Control Department’s (PCAPCD) “Asbestos Removal Test”. A list of accredited training programs can be obtained from the PCAPCD

**40 CFR 61.145(b)(1)(2)(3)(i-iv)** - If asbestos containing material is present in the area to be demolished or renovated, Plume County form AS-2 “DEMOLITION/RENOVATION/ASBESTOS PROJECT NOTIFICATION FORM” must be submitted to the Plume County Air Pollution Control Department (PCAPCD) one month before the demolition or renovation is commenced.

**40 CFR 61.145(c)(3)** - All asbestos material must be wet before removal. Upon removal, all asbestos material must be placed in plastic bags labeled “CONTAINS ASBESTOS MATERIAL” and be wet to the touch.

**40 CFR 61.45(b)(4)(xii)**- All asbestos material from a demolition or renovation project must be disposed of in a certified landfill. A list of certified landfills can be obtained from the PCAPCD.

**40 CFR 61.145(4)(v)** - Asbestos containing material shall be determined by PCAPCD Test Method 17.